As of August 2022, you have six CPL Solo models to choose from.

**Models I, II, IV & VI are for strong and weak emission samples.** They have the best detectors for their given ranges.

**Models III & V are low-cost alternatives to IV and VI**. They have the penultimate detector. The sensitivity difference is 100-1000 fold less than the more expensive IV and VI.

Models III and V are successful with strongly emissive samples; models IV and VI are for a wider range of signal strengths.

*OLIS CPL Solo I* ***350-800 nm***

*OLIS CPL Solo II*  ***400-1100 nm***

OLIS CPL Solo III  **800-1700 nm**

*OLIS CPL Solo IV*  ***800-1700 nm***

OLIS CPL Solo V  **1100-2700 nm**

*OLIS CPL Solo VI*  ***1100-2700 nm***

